**WARRANTY OF**

**FUNDERMAX RESISTANCE²**

The FUNDERMAX RESISTANCE² Warranty is subject to the terms and conditions of sale and delivery of FUNDERMAX unless otherwise stipulated hereinafter. FUNDERMAX warrants for a period of 10 years the quality of FUNDERMAX RESISTANCE² in relation to entire projects and in conformity with the specifications (physical properties) in effect at the time the sales contract is concluded. For a duration of 10 years from the date of delivery, FUNDERMAX shall replace free of charge such FUNDERMAX RESISTANCE² products which can be proved by the customer not to have complied with these specifications at the date of delivery. In the event FUNDERMAX RESISTANCE² material cannot be re-delivered by FUNDERMAX for any reason, FUNDERMAX will supply material that comes as close as possible to the original one.

We expressly exclude any damage going beyond same, in particular consequential damage from defects such as loss of profit, expenses for de-installation and re-installation etc.

FUNDERMAX RESISTANCE² meets the requirements of SEFA3 (24 chemical test) and EN438, additionally an increased resistance to surface wear of 450 revolutions for Uni colours is guaranteed.

FUNDERMAX shall warrant only such panels as have not suffered damage on account of incorrect or careless storage, machining, application, or handling. FUNDERMAX shall expressly not be liable for defective subconstructions or installation, as these are outside our influence.

Machining and installation must conform to FUNDERMAX Technical Information Brochures.

Any warranty claims shall be subject to the following pre-conditions:

* project data sheet – return of completed project data sheet to FUNDERMAX, and confirmation by FUNDERMAX;
* payment in full of claimed goods;
* presentation of purchasing and delivery documents;
* immediate written information / documentation of type and size of damage;
* an acceptable period of time for the inspection of the damage must be granted;
* adherence to local building regulations.

FUNDERMAX will deny any claims that are not related to its material.

Replacement of goods shall not renew the above warranty period.

The conditions of warranty are subject to Austrian Law, excluding the UN Convention on Contracts for the International Sale of Goods.

Exclusive place of jurisdiction shall be Klagenfurt, Austria.

**PROJECT DATA SHEET FOR**

**FUNDERMAX RESISTANCE²**

For the acceptance of the extended warranty on FUNDERMAX RESISTANCE² materials, the presentation of this duly signed project data sheet is mandatory.

It shall be completed by the companies involved in the project, returned to FUNDERMAX and endorsed by FUNDERMAX. This data sheet is the basis for granting the extended warranty for the project below, as executed with FUNDERMAX RESISTANCE² material.

Project No.: Date of Issue:

Recipient: Click or tap here to enter text.

Construction Period: Click or tap here to enter text.

Project Name: Click or tap here to enter text.

Address, country: Click or tap here to enter text.

Planning Office: Click or tap here to enter text.

Construction Company: Click or tap here to enter text.

Dealer: Click or tap here to enter text.

Material/Decor: Click or tap here to enter text.

Quantity: Click or tap here to enter text.

Confirmation by the Construction Company of notice and acceptance (prior to commencement of construction) or adherence (after completion of construction) to the FUNDERMAX Technical Information Brochures:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date, place, company stamp, name, signature (of construction company)

Endorsed by FUNDERMAX:

i.A. Matthias Kauer i.A. Application Engineering

----------------------------------- -----------------------------------